RISK ASSESSMENT – EAST DEAN CHURCH
	Area  - CHANCEL
	
	
	

	Uses / Potential hazards; Communion / Choir / Candles / Steps/
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Fall on Chancel steps going to/from Communion
	Sidesman mans steps to aid 
	1
	2
	2 Low
	None
	
	
	

	Fire risk candles
	Vigilance Wardens & Sidesman. Positioning fire extinguishers
	1
	1
	1 Low
	None
	
	
	

	Hot candle wax burning hands 
	Sideman’s Aide Memoire re extinguishing candles
	1
	1 
	1 Low
	None
	
	
	

	Drilling where necessary[ applies also to Knave; Vestry Open Plan External]
	None
	2
	3
	6 High
	New procedures see Maintenance Policy
	1
	3
	3 Medium




	Area  - VESTRY
	
	
	

	Uses / Potential hazards Robing/ Storage/ Children’s Creche/ Service Preparation/ Photocopying/ Ladder storage/Switch Board
	
	
	

	Hazard / Risk
	Existing Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls 
required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Ladder storage; Children climbing ladder
	Chained barrier board: Children in Cornerstone Room
	1
	2
	2 Low
	None 
	
	
	

	Manoeuvring ladder
	
	2
	2
	4 Medium
	New procedures see Maintenance Policy
	1
	1 
	1 Low

	Work in Tower risk falls and dropping objects
	None
	2
	3
	6 High
	New procedures see Maintenance Policy
	1
	2
	2 Low







	Area  -KNAVE
	
	
	

	Uses / Potential hazards Services/ Pulpit stairs/Slips trips falls/Falls from height/Singing Group electrics
	
	
	

	Hazard / Risk
	Existing Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Fall/trip on Pulpit steps
	Non slip treads on stairs.
Instructions to users
	2
	2
	4 Medium
	Regular Briefing to Ministers and visiting speakers
	1
	2
	2  Low

	“Mobile” step into Curate’s Pew
	None
	2
	3
	6 High
	New step installed with non-slip surface

Now introduce risk now 2:2 Medium
	2
	2
	4  Medium

	Working at Height re Spotlights and Bulbs
	
	2
	3
	6 High
	See HSE Policy re Maintenance Group
New ladder
	1
	3
	3 Medium




	Area  - OPEN PLAN & BAPTISTRY
	
	
	

	Uses / Potential hazards Food & Drink consumption/ baptisms/ Discussion Groups/ Chairs stacked/Bookcase
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	None identified
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	





	Area  - KITCHEN
	
	
	

	Uses / Potential hazards Food & Drink Preparation/ Kitchen utensils/ Oven & Hob/ Fire Risks/ Coffee maker/ Children’s activities/ Toilet/ Entrance, Exit to Churchyard
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Coffee maker – risk scalds and burns if topples
	None
	2
	2
	4 Medium
	See new Food Preparation Policy incls siteing and instructions not for use
	1
	2
	2  Low

	Burns & Scalds Oven/Hob
	Kitchen gate child proof
	2
	3
	6 High
	See Cornerstone Room Policy
	1
	3
	3 Medium

	Fire Hazards
	See Fire Precautions report
	
	
	
	Extinguishers now inplace + Fire blanket
	
	
	

	Children’s activities in Cornerstone Room
	Children to be supervised by leaders and not allowed in the kitchen area
	2
	2
	4Medium
	See Cornerstone Room policy
	1
	2
	2Low




	Area  - BOILER ROOM
	
	
	

	Uses / Potential hazards
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Slippery Steps
	Regular clearance fallen leaves
Access by authorised users only
	1
	3
	3 Medium
	Install hand rail?
	
	
	

	
	
	
	
	
	
	
	
	




	Area  - CHURCHYARD
	
	
	

	Uses / Potential hazards Slip Trip fall Graves open/ Trees falling branches/ Gardening and strimming use of inflammables & pesticides
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Cuts and injuries from using strimmer
	None
	2
	2
	 4 Medium
	Operator to be supplied with PPE
Gloves Mask Ear protection

	1
	2
	2 Low

	Falling Branches
	See Policy on Tree maintenance
	1
	2
	2 Low
	None
	
	
	

	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	




	Area  - PATHS AND ENTRANCES
	
	
	

	Uses / Potential hazards Slip Trip Fall
	
	
	

	Hazard / Risk
	Exisiting Controls
	Likelihood
[1-3]
	Severity
[1-3]
	Risk rating
	Additional Controls required
	Revised 
Likelihood
	Revised 
Severity
	Risk Rating

	Slips & Falls ;Uneven or poorly maintained paving
	Non plan
	3
	2
	6 High
	See Cleaning & Maintence Plan agreed Re-pointing loose mortar
Regular report from “openers” on condition
Hazard Warning signs
Algae Removal 2 x pa
	2
	2
	4 Medium

	Open graves
	Protected by grave digger
	1
	1
	1 Low
	None
	
	
	

	Path Cleaning using electrical pressure washer – Risks to operator and path users
	None
	2
	3
	6 High
	New procedures see Maintenance Policy plus warning signage
	1
	3
	3 Medium



